|  |
| --- |
|  |

 **TECHNICAL BID OF : (***Firm Name***)\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**PROJECT : 67/2020-21 – SUPPLY & INSTALATION OF QUANTITY 4 BUNK BED FOR ARMY INSTITUTE OF MANAGEMENT NEW CAMPUS AT RAJARHAT, KOLKATA**

*1. Please attach supporting drawings, technical literature / brochure, scanned documents / proof etc as applicable.*

*2. Vendors should be prepared to produce product sample(s) on demand within reasonable time – 10 days.*

*3. The bid preferably be typed on letter head of the firm and authenticated by office stamp & signature on each page.*

|  |  |  |  |
| --- | --- | --- | --- |
| S No  | Required Specifications /Parameters / Terms & Conditions | Specifications of Bidder / Compliance Endorsement | Remarks |
| 1. | BUNK BED(a)Frame Size: 6 ½ ’x 3’ (16 swg rectangular tube) and 1”x1” square tube(b)Plywood Thickness – 12mm (c)Head side Leg side made by 48 dia pipe16swg and 1’ dia pipe(d)Ladder will be Leg Side so as to prevent the shortage of space.(e)Top will be Protected with Railing(f)With Shoe Rack in between two Storage(g)Pipes will be round which will lessen the chances for scratches (h)Black colour Powder coating paint |  |  |
| 2. | Registration / Trade License / ROC |  | Please attach self attested proof |
| 3. | GST / TIN  |  | Please attach self attested proof |
| 4. | Earnest Money |  | Please attach instrument details |
| 5. | PAN Card |  | Please attach self attested PAN Card |
| 6. | MSME Registration (If applicable) |  | Please attach self attested proof |
| 7. | Company Profile – quality certification, turnover, tax filings etc (Optional) |  | Please furnish details & attach relevant documents |
| 8. | PoC Contact Particulars |  | Name, Mob No, Email ID |

Date : Signature

 **COMMERCIAL BID OF : (***Firm Name***)\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**PROJECT : 67/2020-21 – SUPPLY & INSTALATION OF QUANTITY 4 BUNK BED FOR ARMY INSTITUTE OF MANAGEMENT NEW CAMPUS AT RAJARHAT, KOLKATA**

*1. The bid preferably be typed on letter head of the firm and authenticated by office stamp & signature on each page.*

*2. Rate quoted should be inclusive of transportation, freight, cartage, handling, fabrication / construction, installation, testing and commissioning at the indicated site (Rajarhat Campus), warranty / guarantee liability costs, taxes and levies and any special requirements given in the tender document.*

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| S No  | Brief Description / Specifications of Job / Work / Product) or Item(s) | Accounting Unit | Quantity | Rate(Rs) | Amount(Rs) | Remarks |
| 1. | BUNK BED(a)Frame Size: 6 ½ ’x 3’ (16 swg rectangular tube) and 1”x1” square tube(b)Plywood Thickness – 12mm (c)Head side Leg side made by 48 dia pipe16swg and 1’ dia pipe(d)Ladder will be Leg Side so as to prevent the shortage of space.(e)Top will be Protected with Railing(f)With Shoe Rack in between two Storage(g)Pipes will be round which will lessen the chances for scratches (h)Black colour Powder coating paint | Nos  | 04 |  |  |  |
| 2. | Overheads / Additionalities(a) Freight(b) Installation | - |  |  |  |  |
|  | Total |  |  |  |  |  |
|  | GST |  |  |  |  |  |
|  | Grand Total |  |  |  |  |  |

Date : Signature